|  |  |
| --- | --- |
| **Software Name:** | Spiking Scheme |
| **Current Version:** | Version 4.1 |
| **Updated Version:** | Version 2 |

**Section 1 – Change Requests(s)**

**Change Request**

|  |
| --- |
| **Description of Change(s)**:  Added carrier dimensions for 0.5mL tube. Drop-down option for 0.5mL tube was added and enabled into the Excel Spiking Macro |

**Halt in Production**: Yes  No

**Change Type (check all that apply)**:

Method Update  Improve Performance  Scope Increase  Cosmetic Change

Bug Fix

|  |
| --- |
|  |

Other

**Impact and Testing Strategy**

|  |
| --- |
| **Testing Strategy**:Updated spiking scheme was run on the Hamilton both in simulation and as a water run. Both runs were successful with the labelled run located here:  T:\BPS\General\Equipment\EQ1846 (Hamilton Starlet)\TEST Macro\TrainingEdStandardSpikes 24-Sep-2021 01 14 PM |

**Back Out Strategy**

|  |
| --- |
| **Back Out Strategy**:  Revert to previous version  Other |

|  |
| --- |
| **Other Comments**: |

**Approval of the Change Request**

|  |  |
| --- | --- |
| **Approver**  **Initial and Date** |  |